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Appendix A.2
Pole-Covered Trench Shelter

PROTECTION PROVIDED

Against fallout radiation: Protection Factor 300
(PF 300)-—a person in the open outside this shelter
would receive 300 times more fallout radiation than
he would if he were inside.

Against blast: Quite good protection if built in
stable earth. Blast tests have indicated that this
shelter, if built in stable earth, would not be seriously
damaged by blast effects of large explosions at least
up to the 7-psi overpressure range. (At 7 psi, most
buildings would be demolished.) Without blast
doors, occupants of the shelter could be injured,
although probably not fatally.

Against fire: Excellent, if sufficiently distant
from fires producing carbon monoxide and toxic
smoke.

WHERE PRACTICAL

In wooded areas with small trees, for builders
who have an ax or a bow saw, crosscut or chain saw,
and digging tools. Or in any location where the
necessary poles may be obtained.

In stable earth, where the water table or rock is
more than 4, ft below the surface.

FOR WHOM PRACTICAL

For a family or other group with two or more
members able to work hard for most of 2 days.

CAPACITY

The shelter illustrated is the minimum length
recommended for 4 persons. For each additional

person, add at least 2%, ft to the length of the shelter
room. If more than about 10 persons are to be
sheltered, build 2 or more separate shelters.

BUILDING INSTRUCTIONS

1. Before beginning  work, study the drawings
and read ALL of the following instructions.
Divide the work so that some people will be
digging while others are cutting and hauling
poles. CHECK OFF EACH STEP WHEN
COMPLETED.

2. By the time the shelter is finished, plan to have
completed: (1) a ventilating pump, and (2) the
storage of at least 15 gallons of drinking water
per occupant (see Appendix B and Chapter 8).

3. Start to assemble materials and tools. Those
listed are for the illustrated 4-person shelter with
a room 11 ft long.

A. Essential Materials and Tools

® Saw (bow saw or crosscut preferred)
and/or ax for cutting poles to the lengths and
diameters illustrated.

® Shovels (one for each two workers).

®  Pick (if the ground is hard).

® Rainproof roof materials (very impor-
tant in rainy, cold weather). At least 2 square
yards of such material per person would be
required; 3 square yards per person would be
better. Shower curtains, plastic tablecloths,
plastic mattress covers, canvas, and the like
can be used. Also needed are 2 pieces of
plastic or tightly woven cloth, each about
6", X 6', ft, to make canopies over the two
shelter openings.

®  Materials and tools for building a simple
shelter-ventilating pump, a KAP 22 in. wide
and 36 in. long. (See Appendix B.) Only in
cold or continuously breezy, cool weather

133






[image: image5.png]134

can tolerable temperatures and humidities be
maintained for days in a crowded under-
ground shelter that lacks an air pump.

® Containers for storing adequate water.
(See Chapter 8.)

B. Useful Materials and Tools

® large cans, buckets, and/or pots with

hail handlee—in which ¢
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later to store drinking water and human
wastes.

® Two bedsheets and two pillowcases per
person for covering cracks between roofing
logs, making “sandbags,” and improvising
bedsheet-hammocks and bedsheet-chairs.

® A file.
® A measuring tape, yardstick, or ruler.

® Rope, or strong wire (100 ft)—to make
earth-retaining pole walls close to the shelter
openings (as explained in step 19) and for
hammock supports, etc.

® Chain saw, pick-mattock, hammer,
hatchet, pliers.

® Kerosene, turpentine, or oil—to keep
hand saws from sticking in gummy wood.

® FExpedient life-support items recom-

mended in this book.

®  Mosquito netting or window screen to
cover the openings, if mosquitoes or flies are
likely to be a problem.

QOIT A DYDIERT

. To save time and work, SHARPEN ALL

TOOLS AND KEEP THEM SHARP.

Wear gloves from the start—even tough hands
can blister after hours of chopping and digging,
and become painful and infected.

If possible, select a location for the shelter that is
in the open and at least 50 ft from a building or
woods. Remember that on a clear day the
thermal pulse (flash of heat rays) from a very
large nuclear explosion may cause fires as far
away as 25 miles.

If the site chosen is on a steep slope, locate the
shelter with its length crosswise to the direction
of the slope.

10.

1.

12.

13.

14.

15.

. Stake out the outlines of the trench, driving

stakes as indicated in Fig. A.2.1 at the end of
Appendix A.2. If more than 4 persons are to be
sheltered, increase the length of the shelter room
by 2 ft 9 in. for each additional person.

Clear the ground of saplings and tall grass within
10 ft of the staked outlines so that later the
excavated earth can be easily shoveled back onto
the completed shelter roof.

Start digging, throwing the first earth about 10 ft
beyond the staked outlines of the trench. Less
able members of the family should do the easier
digging, near the surface. Those members who
can use an ax and saw should cut and haul poles.
See the introductory section of this appendix for
the know-how to make this hard work easier.

Pile all excavated earth at least 2 ft beyond the
edges of the trench, so roofing poles can be laid
directly on the ground. To make sure that the
trenches are dug to the specified full widths at the
bottoms, cut and use two sticks-—one 42 in. long
and the other 22 in. long——to check trench widths
repeatedly.

At the far end of the shelter dig the ventilation
trench-emergency exit, making it 22 in. wide and
40 in. deep. This will help provide essential
ventilation and cooling. In cold weather or when
........................

should be hung in the two openings to controlthe
air flow.

Make and install threshold boards, to keep the
edges of earth steps and earth ledges from being
broken off. (In damp earth, it is best to install
threshold boards before roofing the shelter.) If
boards are lacking, use small poles.

Unless the weather is cold, build a shelter-
.............

high. (If the weather is cold, building a KAP can
be safely delayed until after the shelter is
completed.) A KAP should be made before a
crisis, or, if possible, before leaving home.

Obtain fresh-cut green poles, or, as a second
choice, sound, dry, untreated poles. Use no poles
smaller in diameter than those specified in the
accompanying drawings. For ease in hauling,
select poles no more than 509 larger in diameter
than those specified.
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Lay the poles side by side over the trench.
Alternate the large and small ends to keep the
poles straight across the trench. If roof poles 9 ft
long are being used to roof a 5-ft-wide trench, be

sure to place the roof poles so that their ends

extend 2 ft farther bpynnd one side nf the trench

than beyond the other side. This will enable
shelter occupants, after the stoop-in shelter is
completed, to widen the shelter room 2 ft on one
side. First, it can be widened to provide a 2-ft-
wide sleeping ledge. Later, it can be further
deepened to make space for additional expedient
hammocks or for double-bunk beds of poles or
boards built on each side of the shelter.

For ease and safety later when hanging expedient
bedsheet-hammocks and bedsheet-chairs in the
completed shelter, place loose loops around roof
poles in the approximate locations given by the
diagram on the second shelter drawing, Fig.
A.2.2. Make these loose loops of rope, or strong
wire, or 16-in-wide strips of strong cloth, such as
509 polyester bedsheet rolled up to form a
“rope”. (For making hammocks and seats, see
Chapter 14. These are not essential, although
decidedly useful.)

Cover the cracks between the logs with cloth,
leaves, clay, or any other material that will keep
dirt from falling down between the cracks.
CAUTION: DO NOT try to rainproof this flat
roof, and then simply cover it with earth. Water
will seep through the loose earth cover, puddle
on the flat roofing material, and leak through the
joints between pieces of roofing material or
through small holes.

Place 6-ft-long poles, one on top of the other,
next to the entrances. This will keep earth to be
placed on top of the entryway trenches from
falling into the openings. Secure these poles with
wire or rope. (See View A-A’ in Fig. A.2.1.) If
wire or rope is not available, make earth-filled
“rolls” to hold the earth nearly vertical on the
trench roof next to each opening. (See the
introductory section of this appendix.)

Mound earth to a center depth of about 18 in.
over the shelter roof (as shown in View B-B' in
Fig. A.2.1) to form the surface of the future
“puried roof.” Be sure io siope both sides of the
mound. Then smooth its surface and remove
sharp roots and stones that might puncture thin
rainproofing materials to be placed upon it.

21

22.

23.

24,

25.

26.

27.

28.

(¥e]
wh

Place the waterproofing material on the “buried
roof.” If small pieces must be used, lay them in
shingle-like fashion, starting at the lower sides of
the mounded earth.

Cover the buried roof with another 18 in. of
mounded earth, and smooth this final earth
surface.

Finish the entrances by placing some shorter
poles between the two longer poles next to each
entryway. Bank and pack earth at least 6 in. deep
around the sides of the entrances, so that
rainwater on the ground cannot run into the
shelter entrances.

Dig surface drainage ditches around the outside
of the mounded earth and around the entrances.

Place a piece of water-shedding material over
each of the entrances, forming an open-ended
canopy to keep fallout and rain from the shelter
openings. (See Fig. A in the introductory section
of Appendix A.) Almost all fallout would settle
on these suspended canopies, rather than falling
into shelter openings—or would fall off their
edges and onto the ground like sand.

Hang the KAP from the roof of the trench
opening into which outdoor air can be felt
flowing, so that air will be pumped in the
direction of the natural flow of air.

Fill all available water containers, including pits
which have been dug and lined with plastic, then
roofed with available materials. If possible,
disinfect all water stored in expedient containers,

using one scant teaspoon of a chlorine bleach,

such as Clorox, for each 10 gallons of water.
Even if only muddy water is available, store it. If
you do not have a disinfectant, it may be possible
to boil water when needed.

As time and materials permit, continue to
improve your chances of surviving by doing as
many of the following things as possible;

(1) Make a homemade fallout meter, as de-
scribed in Appendix C.

(2) Make expedient lights.

(3) Make and hang expedient bedsheet-
hammocks and bedsheet-chairs, following
the installation diagram shown in Fig. A.2.2.

(4) Install screens of mosquito netting over the
two openings, if mosquitoes or flies are a
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problem. Remember, however, that screen
or netting reduces the air flow through a

shelter—even when the air is pumped
through with a KAP.

(5) Dig a stand-up hole near the far end of the
shelter. Make the hole about 15 in. in
diameter and deep enough to permit the
tallest of the shelter occupants to stand erect
occasionally.
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