FSJ Engine Codes 360 V8

Contributed By: Joe Schaefer 

The six digit Engine Code is stamped on a metal tag on the front of the right Valve Cover. 

1st Digit - Year 

	4- 1971

	5- 1972

	6- 1973

	7- 1974

	8- 1975

	9- 1976

	1- 1977

	2- 1978

	3- 1979

	0- 1980

	1- 1981

	2- 1982 etc.


2nd & 3rd Digit - Month 

4th Digit - Type 

	N- V8-360 2V 

	P- V8-360 4V

	NX- V8-360/5.9L w/2V carb, 1987 and later. 


5th & 6th Digit - Day 

Note 1: Applicable only up to 1986, odd engine size characteristics will be stamped to the upper half of the Engine Code Plate as follows: 
	B- 0.010" Oversize Cylinder Bore

	C- 0.010" Oversize Camshaft Bores

	M- 0.010" Undersize Main Bearings

	P- 0.010" Undersize Wrist Pins

	PM- 0.010" Undersize Wrist Pins and Main Bearings


Note 2: Engines built for sale in Georgia or Tennessee from 1987 on have an additional non-repeating number above the build date code. 

References: 

	Jeep Engine, Chassis, and Body Service Manual 25M888, 1989 JEEP Vehicles, copyright 1988 Jeep/Eagle Corporation.

	Parts Manual: W-1170-R2, Kaiser Jeep Corporation, 1967

	Parts Manual: F-76072, AMC, Feb 1972

	Parts Manual: F-75080, AMC, May 1980

	Parts Manual: 89-81-374-084, AMC, May 1987


